1. Install JRE 1.8.0\_151 from link below  
   <http://www.oracle.com/technetwork/java/javase/downloads/jre8-downloads-2133155.html>
2. Install Master Device (ESP8266 NodeMCU) driver on Admin machine  
   <https://www.silabs.com/products/development-tools/software/usb-to-uart-bridge-vcp-drivers>
3. Make sure you have Chrome Browser, Or install Chrome
4. Connect the Master device with Admin machine using a USB
5. Power The Client Device  
   Wait for the device to connect network, RGB will turn Blue -> Green and finally Off
6. Unzip Admin\_SW.zip at Desktop
7. Open Admin\_SW folder, Right Click “Start.jar” and Open  
     
   It will open a Chrome and another application to establish connection between master device and Admin machine
8. On the Application, select port of the master device, Click “OPEN PORT” button

Note:

* There will no data on Dashboard initially
* The Page will automatically refresh every Two minutes
* Do not refresh the Page manually